## Command-Line Options

User's Guide > Operation > Command-Line Options

-f -freq ???
  Sampling frequency in Hz.
  Example:

            spwave -f 8000 data_8k.ad

  In this example, data_8k.ad will be loaded with 8kHz sampling frequency.
-F -format ???
  File format. See Format for more information.

  Example:

            spwave -format swap data_swap.ad

  In this example, data_swap.ad will be loaded with swap format.

-c -channel ???
  Number of Channels.
  Example:

            spwave -channel 8 data_8channel.ad

  In this example, data_8channel.ad will be loaded with 8 channels data format.
-b -bit bits_per_sample
  Bits/sample. For example. `short' type in C language is 16 bits/sample. For more information, see Format.

  Example:

            spwave -bit 64 data_64bit.ad

  In this example, data_64bit.ad will be loaded with 64 bits/sample data format.

-h -help
  Diplay help messages.

User's Guide > Operation > Command-Line Options

Last modified: "2012-08-22 01:33:00 hideki"